{"text_format":"3","workbook":"xls","n_sheets":10,"sheets":["废气有组织","废气有组织 (2)","废气无组织","厂界噪声","废水","周边环境质量（海创）","比对监测","油烟监测","个人剂量监测","皮带探伤设备辐射检测"],"not_rendered":{"images":3,"external_links":1,"defined_names":10,"comments":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气有组织","index":0,"n_rows":100,"n_cols":18,"rows_kept":100,"merged":[[0,0,0,17],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[1,8,3,8],[1,9,3,9],[1,10,3,10],[1,11,3,11],[1,12,3,12],[1,13,3,13],[1,14,3,14],[1,15,3,15],[1,16,3,16],[1,17,3,17],[75,0,85,0],[75,1,85,1],[75,3,85,3],[75,6,85,6],[75,7,85,7],[75,8,85,8],[75,9,85,9]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（有组织废气）"]
["序号","污染治理设施名称","设备型号","排口编号","监测内容","污染物","设计处理风量   （Nm3/h)","排气筒高度(m)","排气筒出口内径(m)","排口类型","限值(mg/Nm3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[]
[]
[1,"7#8#机器人车道废气排放口",null,"DA001","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",38860,15.2,0.82,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[2,"1#机器人车道废气排放口",null,"DA002","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",30553,9.73,0.82,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[3,"石灰石破碎机废气排放口",null,"DA003","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",27757,15,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[4,"砂岩破碎机废气排放口",null,"DA005","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",27757,15.5,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[5,"石灰石出料转运站皮带废气排放口",null,"DA007","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9636,17,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[6,"石灰石长皮带尾部废气排放口",null,"DA008","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9636,37.3,0.56,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[7,"砂岩出料转运站废气排放口",null,"DA009","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8855,20.7,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[8,"1#包装机废气排放口",null,"DA010","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,20.5,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[9,"1、2#散装水泥发运斗提振动筛废气排放口",null,"DA011","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[10,"1#水泥包装机斗提下废气排放口",null,"DA012","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[11,"4#机器人车道废气排放口",null,"DA013","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,9.73,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[12,"2#水泥包装机斗提下废气排放口",null,"DA014","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[13,"3#水泥包装机斗提下废气排放口",null,"DA015","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[14,"4#水泥包装机斗提下废气排放口",null,"DA016","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[15,"1#水泥粉磨调配秤废气排放口",null,"DA017","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[16,"2#水泥粉磨调配秤废气排放口",null,"DA018","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[17,"1#水泥入库斗提废气排放口",null,"DA019","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,33,0.37,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[18,"煤粉仓废气排放口",null,"DA020","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",7410,40,0.29,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[19,"2#水泥入库斗提废气排放口",null,"DA022","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,33,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[20,"1#水泥库下包装1#斜槽废气排放口",null,"DA023","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,15,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[21,"1#水泥库下散装斜槽废气排放口",null,"DA024","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11.5,0.29,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[22,"4#水泥库下1#包装斜槽废气排放口",null,"DA025","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11.5,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[23,"#水泥库下2#包装斜槽废气排放口",null,"DA026","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11.5,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[24,"4#水泥库下散装斜槽废气排放口",null,"DA027","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,11.5,0.29,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[25,"水泥粉磨磨头熟料仓废气排放口",null,"DA028","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,18,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[26,"水泥粉磨磨头石灰石仓废气排放口",null,"DA029","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,18,0.52,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[27,"1#包装机中间仓废气排放口",null,"DA030","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,27.5,0.46,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[28,"2#包装机中间仓废气排放口",null,"DA031","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,27.5,0.46,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[29,"3#包装机中间仓废气排放口",null,"DA032","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,27.5,0.46,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[30,"4#包装机中间仓废气排放口",null,"DA033","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,27.5,0.46,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[31,"联合储库出库皮带废气排放口",null,"DA034","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[32,"2#包装机废气排放口",null,"DA035","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,20.5,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[33,"3#包装机废气排放口",null,"DA036","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,20.5,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[34,"4#包装机废气排放口",null,"DA037","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,20.5,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[35,"1#散装水泥装车机废气排放口",null,"DA038","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[36,"2#散装水泥装车机废气排放口",null,"DA039","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[37,"3#散装水泥装车机废气排放口",null,"DA040","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[38,"4#散装水泥装车机废气排放口",null,"DA041","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[39,"5#散装水泥装车机废气排放口",null,"DA042","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[40,"6#散装水泥装车机废气排放口",null,"DA043","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,10,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[41,"水泥粉磨入磨头仓辅材破碎机转运站皮带废气排放口",null,"DA044","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,18,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[42,"水泥粉磨入磨头仓辅材跨河转运站皮带废气排放口",null,"DA045","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[43,"3#石灰石出库皮带废气排放口",null,"DA046","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,22,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[44,"2#石灰石出库皮带废气排放口",null,"DA047","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[45,"1#石灰石出库皮带废气排放口",null,"DA048","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[46,"1#、2#包装皮带机废气排放口",null,"DA049","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,10,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[47,"5#6#机器人车道废气排放口",null,"DA050","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",30533,9.73,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[48,"7、8#袋装水泥装车道废气排放口",null,"DA051","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,10,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[49,"砂岩入联合储库皮带废气排放口",null,"DA052","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9636,24.5,0.46,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[50,"粉煤灰库废气排放口",null,"DA053","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8900,43,0.52,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[51,"1、6#号水泥库废气排放口",null,"DA054","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,55,0.63,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[52,"2、5#号水泥库废气排放口",null,"DA055","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,55,0.62,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[53,"3、4#号水泥库废气排放口",null,"DA056","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,55,0.62,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[54,"1#水泥散装仓废气排放口",null,"DA057","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,32,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[55,"2#散装水泥仓废气排放口",null,"DA058","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,32,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[56,"3#水泥散装仓废气排放口",null,"DA059","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,32,0.28,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[57,"1#水泥磨废气排放口",null,"DA060","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物","主收尘：240000\n尾收尘：53000",35,2.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[58,"2#水泥磨废气排放口",null,"DA061","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物","主收尘：240000\n尾收尘：53000",35,2.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[59,"熟料散装仓废气排放口",null,"DA062","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,25,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[60,"生料均化库顶废气排放口",null,"DA064","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",13848,65,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[61,"原料石灰石调配库废气排放口",null,"DA065","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,30,0.51,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[62,"熟料库顶废气排放口",null,"DA066","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",13848,45,1,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[63,"窑头废气排放口",null,"DA067","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",580000,40,3.6,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","每天不少于4次，每次间隔不超过6小时.自动监测设备出现故障，采用手工监测。","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",null,"季度监测时，在委托报告上体现监测数据"]
[64,"石膏破碎机废气排放口",null,"DA068","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,13,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[65,"熟料库地坑1#出库皮带废气排放口",null,"DA069","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.62,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[66,"熟料库地坑1#转运站皮带废气排放口",null,"DA070","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.57,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[67,"熟料库地坑2#出库皮带废气排放口",null,"DA071","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.62,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[68,"熟料库地坑2#转运站皮带废气排放口",null,"DA072","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.56,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[69,"熟料库地坑3#出库皮带废气排放口",null,"DA073","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.62,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[70,"熟料库地坑3#转运站皮带废气排放口",null,"DA074","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[71,"熟料出地坑皮带（1716）废气排放口",null,"DA075","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9300,25,0.63,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[72,"窑尾废气排放口",null,"DA076","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",785000,90,6,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","每天不少于4次，每次间隔不超过6小时","非连续采样 至少3个","固定污染源废气  低浓度颗粒物的测定-重量法 HJ 836-2017",null,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","二氧化硫",{"$nulls":4},200,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","每天不少于4次，每次间隔不超过6小时","非连续采样 至少3个","固定污染源排气中二氧化硫的测定 定电位电解法HJ 57-2017, 固定污染源废气 二氧化硫的测定 便携式紫外吸收法（HJ 1131-2020）",null,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","氮氧化物",{"$nulls":4},350,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","每天不少于4次，每次间隔不超过6小时。自动监测设备出现故障，采用手工监测。","非连续采样 至少3个","固定污染源废气 氮氧化物的测定 定电位电解法HJ 693-2014, 固定污染源废气  氮氧化物的测定 便携式紫外吸收法（HJ 1132-2020）",null,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","汞及其化合物",{"$nulls":4},0.05,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","固定污染源废气 汞的测定 冷原子吸收分光光度法 (暂行)HJ 543—2009",8]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","氨（氨气）",{"$nulls":4},10,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样 至少3个","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",8]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","氯化氢（HCl)",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样 至少3个","固定污染源废气 氯化氢的测定 HJ 549-2016",4,"梁平海创"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","氟化氢（HF)",{"$nulls":4},{"v":1,"d":"1.0"},"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样 至少3个","固定污染源废气 氟化氢的测定 离子色谱法HJ 688-2019",4,"梁平海创"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物",{"$nulls":4},0.5,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样 至少3个","空气和废气 颗粒物中铅等金属物的测定 电感耦合等离子体质谱法HJ657-2013及修改单",4,"梁平海创"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","铊、镉、铅、砷及其化合物",{"$nulls":4},{"v":1,"d":"1.0"},"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样 至少3个","空气和废气 颗粒物中铅等金属物的测定 电感耦合等离子体质谱法HJ 657-2013及修改单",4,"梁平海创"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","总有机碳",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样 至少3个","固定污染源废气 总烃 甲烷和非甲烷总烃的测定 气相色谱法 HJ38-2017",4,"梁平海创"]
[{"$nulls":4},"烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","二噁英",{"$nulls":4},"0.1ng-TEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/年","非连续采样 至少3个","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱－高分辨质谱法HJ 77.2－2008",2,"梁平海创"]
[73,"煤磨主收尘器废气排放口",null,"DA077","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",105000,40,2,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[74,"石灰石堆场出库废气排放口",null,"DA078","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,15,0.51,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[75,"入石灰石调配库转运站废气排放口",null,"DA079","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,34.4,0.51,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[76,"原煤卸车地坑废气排放口",null,"DA080","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[77,"入煤堆场皮带废气排放口",null,"DA081","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,15,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[78,"出煤堆场1#皮带废气排放口",null,"DA082","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,25,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[79,"出煤堆场2#皮带废气排放口",null,"DA083","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",9639,35,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[80,"生料输送主斜槽废气排放口",null,"DA084","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8855,16,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[81,"生料均化库底斜废气排放口",null,"DA085","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",12166,25,0.57,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[82,"1852出生物质破碎机皮带废气排放口",null,"DA089","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",8928,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/季","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",8,"对于采用相同种类治理设施的，采取随机抽测原则，每次抽测比例不少于 50%。"]
[83,"1859出步进输送仓皮带废气排放口",null,"DA090","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",6696,22,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[84,"1878缓冲仓顶废气排放口",null,"DA091","烟气流速,烟气温度,烟气压力,烟气含湿量,烟道截面积,氧含量,烟气量","颗粒物",6696,60,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工","1次/两年","非连续采样 至少3个","《固定污染源废气低浓度颗粒物的测定-重量法》（HJ836-2017）",1]
[null,"合计",{"$nulls":14},197]
[{"$nulls":16},197]

{"sheet":"废气有组织 (2)","index":1,"n_rows":103,"n_cols":12,"rows_kept":103,"hidden":true,"merged":[[0,0,0,11],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[1,8,3,8],[1,9,3,9],[1,10,3,10],[1,11,3,11],[77,0,87,0],[77,1,87,1],[77,2,87,2],[77,3,87,3],[77,4,87,4],[77,6,87,6],[97,0,99,0],[97,1,99,1],[97,2,99,2],[97,3,99,3],[97,4,99,4],[97,6,99,6],[100,0,102,0],[100,1,102,1],[100,2,102,2],[100,3,102,3],[100,4,102,4],[100,6,102,6]],"flags":["formulas_cached_only"]}
["梁平海螺2022年-2023年环境自行监测方案（有组织废气）"]
["序号","污染治理设施名称","设备型号","排口编号","监测内容","污染物","排口类型","限值(mg/Nm3)","执行标准","监测方式","监测频次","监测采样要求"]
[]
[]
[1,"石灰石破碎机废气排放口",null,"DA003","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[2,"骨料破碎机废气排放口",null,"DA004","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[3,"砂岩破碎机废气排放口",null,"DA005","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[4,"骨料筛分机废气排放口",null,"DA006","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[5,"石灰石出料转运站皮带排放口",null,"DA007","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[6,"石灰石长皮带尾部废气排放口",null,"DA008","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[7,"砂岩出料转运站排放口",null,"DA009","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[8,"1#包装机废气排放口",null,"DA010","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[9,"1、2#散装水泥发运斗提振动筛废气排放口",null,"DA011","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[10,"1#水泥包装机斗提下废气排放口",null,"DA012","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[11,"3、4#袋装水泥装车道废气排放口",null,"DA013","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[12,"2#水泥包装机斗提下废气排放口",null,"DA014","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[13,"3#水泥包装机斗提下废气排放口",null,"DA015","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[14,"4#水泥包装机斗提下废气排放口",null,"DA016","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[15,"1#水泥磨调配秤废气排放口",null,"DA017","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[16,"2#水泥磨调配秤废气排放口",null,"DA018","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[17,"1#水泥入库斗提废气排放口",null,"DA019","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[18,"煤粉仓废气排放口",null,"DA020","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[19,"骨料库废气排放口",null,"DA021","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[20,"2#水泥入库斗提废气排放口",null,"DA022","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[21,"1#水泥库下包装1#斜槽废气排放口",null,"DA023","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[22,"1#水泥库下1#散装斜槽废气排放口",null,"DA024","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[23,"4#水泥库下1#包装斜槽废气排放口",null,"DA025","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[24,"1#水泥库下2#包装斜槽废气排放口",null,"DA026","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[25,"4#水泥水泥库下散装斜槽废气排放口",null,"DA027","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[26,"水泥粉磨磨头熟料仓废气排放口",null,"DA028","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[27,"水泥粉磨磨头石灰石仓废气排放口",null,"DA029","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[28,"1#包装机中间仓废气排放口",null,"DA030","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[29,"2#包装机中间仓废气排放口",null,"DA031","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[30,"3#包装机中间仓废气排放口",null,"DA032","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[31,"4#包装机中间仓废气排放口",null,"DA033","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[32,"联合储库出库皮带废气排放口",null,"DA034","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[33,"2#包装机废气排放口",null,"DA035","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[34,"3#包装机废气排放口",null,"DA036","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[35,"4#包装机废气排放口",null,"DA037","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[36,"1#散装水泥装车机废气排放口",null,"DA038","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[37,"2#散装水泥装车机废气排放口",null,"DA039","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[38,"3#散装水泥装车机废气排放口",null,"DA040","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[39,"4#散装水泥装车机废气排放口",null,"DA041","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[40,"5#散装水泥装车机废气排放口",null,"DA042","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[41,"6#散装水泥装车机废气排放口",null,"DA043","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[42,"水泥粉磨入磨头仓辅材破碎机转运站皮带废气排放口",null,"DA044","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[43,"水泥粉磨入磨头仓辅材跨河转运站皮带废气排放口",null,"DA045","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[44,"3#石灰石出库皮带废气排放口",null,"DA046","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[45,"2#石灰石出库皮带废气排放口",null,"DA047","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[46,"1#石灰石出库皮带废气排放口",null,"DA048","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[47,"1、2#袋装水泥装车道废气排放口",null,"DA049","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[48,"5、6#袋装水泥装车道废气排放口",null,"DA050","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[49,"7、8#袋装水泥装车道废气排放口",null,"DA051","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[50,"砂岩入联合储库皮带废气排放口",null,"DA052","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[51,"粉煤灰库废气排放口",null,"DA053","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[52,"1、6#袋装水泥装车道废气排放口",null,"DA054","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[53,"2、5#袋装水泥装车道废气排放口",null,"DA055","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[54,"3、4#袋装水泥装车道废气排放口",null,"DA056","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[55,"1#散装水泥库废气排放口",null,"DA057","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[56,"2#散装水泥库废气排放口",null,"DA058","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[57,"3#散装水泥库废气排放口",null,"DA059","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[58,"1#水泥磨废气排放口",null,"DA060","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[59,"2#水泥磨废气排放口",null,"DA061","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[60,"熟料散装仓废气排放口",null,"DA062","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[61,"纯石库废气排放口",null,"DA063","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[62,"生料均化库顶废气排放口",null,"DA064","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[63,"原料石灰石调配库废气排放口",null,"DA065","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[64,"熟料库顶废气排放口",null,"DA066","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[65,"窑头废气排放口",null,"DA067","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样"]
[66,"石膏破碎机废气排放口",null,"DA068","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[67,"熟料库地坑1#出库皮带废气排放口",null,"DA069","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[68,"熟料库地坑1#转运站皮带废气排放口",null,"DA070","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[69,"熟料库地坑2#出库皮带废气排放口",null,"DA071","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[70,"熟料库地坑2#转运站皮带废气排放口",null,"DA072","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[71,"熟料库地坑3#出库皮带废气排放口",null,"DA073","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[72,"熟料库地坑3#转运站皮带废气排放口",null,"DA074","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[73,"熟料库地坑皮带（1617）废气排放口",null,"DA075","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[74,"窑尾废气排放口",null,"DA076","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样"]
[{"$nulls":5},"二氧化硫",null,200,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样"]
[{"$nulls":5},"氮氧化物",null,350,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样"]
[{"$nulls":5},"汞及其化合物",null,0.05,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样至少3个样"]
[{"$nulls":5},"氨（氨气）",null,10,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/季","非连续采样至少3个样"]
[{"$nulls":5},"氯化氢（HCl)",null,10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样至少3个样"]
[{"$nulls":5},"氟化氢（HF)",null,{"v":1,"d":"1.0"},"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样至少3个样"]
[{"$nulls":5},"铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物",null,0.5,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样至少3个样"]
[{"$nulls":5},"铊、镉、铅、砷及其化合物",null,{"v":1,"d":"1.0"},"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样至少3个样"]
[{"$nulls":5},"总有机碳",null,10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/半年","非连续采样至少3个样"]
[{"$nulls":5},"二噁英",null,"0.1ng-TEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","1次/年","非连续采样至少3个样"]
[75,"煤磨主收尘器废气排放口",null,"DA077","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/半年","非连续采样至少3个样"]
[76,"石灰石堆场出库废气排放口",null,"DA078","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[77,"入石灰石调配库转运站废气排放口",null,"DA079","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[78,"原煤卸车地坑废气排放口",null,"DA080","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[79,"入煤堆场皮带废气排放口",null,"DA081","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[80,"出煤堆场1#皮带废气排放口",null,"DA082","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[81,"出煤堆场2#皮带废气排放口",null,"DA083","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[82,"生料输送主斜槽废气排放口",null,"DA084","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[83,"生料均化库底斜槽废气排放口",null,"DA085","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","颗粒物","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","1次/两年","非连续采样至少3个样"]
[84,"1#活性炭除臭装置",null,"DA086","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","氨（氨气）","一般排放口（应急排放口）","4.9kg/h","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]
[{"$nulls":5},"硫化氢",null,"0.33kg/h","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]
[{"$nulls":5},"臭气浓度",null,"2000（无纲量）","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]
[85,"2#活性炭除臭装置",null,"DA087","烟气流速,烟气温度,烟气含湿量,烟道截面积，烟气压力，烟气量，氧含量","氨（氨气）","一般排放口（应急排放口）","4.9kg/h","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]
[{"$nulls":5},"硫化氢",null,"0.33kg/h","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]
[{"$nulls":5},"臭气浓度",null,"2000（无纲量）","恶臭污染物排放标准GB 14554-93","手工监测","1次/半年（停窑检修应急排放时）","非连续采样至少3个样"]

{"sheet":"废气无组织","index":2,"n_rows":20,"n_cols":12,"rows_kept":20,"merged":[[0,0,0,11],[2,11,19,11]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（无组织废气）"]
["序号","监测位置","监测内容","污染物名称","限值(mg/Nm3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[1,"主厂区东侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8,"因梁平海创环评报告书中明确指出：颗粒物、氨、臭气浓度、硫化氢每季度开展一次自行监测。"]
[2,"主厂区西侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8]
[3,"主厂区南侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8]
[4,"主厂区北侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8]
[5,"主厂区东侧","风速、风向","氨（氨气）",{"v":1,"d":"1.0"},"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",8]
[6,"主厂区西侧","风速、风向","氨（氨气）",{"v":1,"d":"1.0"},"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",8]
[7,"主厂区南侧","风速、风向","氨（氨气）",{"v":1,"d":"1.0"},"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",8]
[8,"主厂区北侧","风速、风向","氨（氨气）",{"v":1,"d":"1.0"},"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",8]
[9,"主厂区东侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 硫化氢 甲硫醇 甲硫醚 二甲二硫的测定气相色谱法 GB/T14678-1993",8]
[10,"主厂区西侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 硫化氢 甲硫醇 甲硫醚 二甲二硫的测定气相色谱法 GB/T14678-1993",8]
[11,"主厂区南侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 硫化氢 甲硫醇 甲硫醚 二甲二硫的测定气相色谱法 GB/T14678-1993",8]
[12,"主厂区北侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 硫化氢 甲硫醇 甲硫醚 二甲二硫的测定气相色谱法 GB/T14678-1993",8]
[13,"主厂区东侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",8]
[14,"主厂区西侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",8]
[15,"主厂区南侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",8]
[16,"主厂区北侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","季度/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",8]
[17,"石灰石矿主采场","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8]
[18,"砂岩矿主采场","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法（HJ 1263—2022）",8]

{"sheet":"厂界噪声","index":3,"n_rows":9,"n_cols":9,"rows_kept":9,"merged":[[0,0,0,8],[2,3,8,3]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（噪声）"]
["序号","监测位置","监测内容","限值(dB)","执行标准","监测方式","监测频次","两年监测次数","备注"]
[1,"主厂区北侧（李家坪居民）","风速、风向","昼间:60dB；           夜间:50dB。","工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[2,"主厂区西侧（近石灰石堆场）","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[3,"主厂区南侧（近混合材堆场）","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[4,"主厂区北侧（厂界外）","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[5,"主厂区北侧（近循环水池）","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[6,"石灰石矿主采场","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[7,"砂岩矿主采场","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]

{"sheet":"废水","index":4,"n_rows":67,"n_cols":11,"rows_kept":67,"merged":[[0,0,0,10],[2,1,9,1],[2,2,9,2],[2,5,9,5],[10,1,17,1],[10,2,17,2],[10,5,17,5],[18,1,25,1],[18,2,25,2],[18,5,25,5],[26,1,33,1],[26,2,33,2],[26,5,33,5],[34,1,43,1],[34,2,43,2],[34,5,43,5],[34,7,43,7],[44,1,53,1],[44,2,53,2],[44,5,53,5],[44,7,53,7],[55,0,55,10],[57,1,66,1],[57,2,66,2]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（废水）"]
["序号","排口编号","监测内容","污染因子","限值(mg/L)","执行标准","监测方式","监测依据及方法","监测频次","两年监测次数","备注"]
[1,"生活区污水处理器（DW001）","流量、水温","pH值","6.0-9.0","污水综合排放标准标准（GB 8978-1996) 表4中一级排放标准","手工监测","水质 pH值的测定 电极法 GB 1147-2020","季度/次",8]
[2,null,null,"悬浮物",70,null,"手工监测","水质 悬浮物的测定 重量法 GB 11901-1989","季度/次",8]
[3,null,null,"五日生化需氧量",20,null,"手工监测","水质 五日生化需氧量（BOD5）的测定 稀释与接种法 HJ505-2009","季度/次",8]
[4,null,null,"化学需氧量",100,null,"手工监测","水质 化学需氧量的测定  重铬酸盐法 HJ828-2017","季度/次",8]
[5,null,null,"氨氮（NH3-N）",15,null,"手工监测","水质 氨氮的测定蒸馏-中和滴定法 HJ537-2009","季度/次",8]
[6,null,null,"总磷（以P计）",0.5,null,"手工监测","水质 总磷的测定 钼酸铵分光光度法 GB 11893-1989","季度/次",8]
[7,null,null,"氟化物",10,null,"手工监测","水质 氟化物的测定 离子选择电极法（GB 7484-87）","季度/次",8]
[{"$nulls":3},"石油类",5,null,"手工监测","水质 石油类和动植物油类的测定 红外分光光度法(HJ 637-2018)","季度/次",8]
[25,"制造分厂污水处理器（DW002）","流量、水温","pH值","6.0-9.0","污水综合排放标准标准（GB 8978-1996) 表4中一级排放标准","手工监测","水质 pH值的测定 电极法 GB 1147-2020","季度/次",8]
[26,null,null,"悬浮物",70,null,"手工监测","水质 悬浮物的测定 重量法 GB 11901-1989","季度/次",8]
[27,null,null,"五日生化需氧量",20,null,"手工监测","水质 五日生化需氧量（BOD5）的测定 稀释与接种法 HJ505-2009","季度/次",8]
[28,null,null,"化学需氧量",100,null,"手工监测","水质 化学需氧量的测定  重铬酸盐法 HJ828-2017","季度/次",8]
[29,null,null,"氨氮（NH3-N）",15,null,"手工监测","水质 氨氮的测定蒸馏-中和滴定法 HJ537-2009","季度/次",8]
[30,null,null,"总磷（以P计）",0.5,null,"手工监测","水质 总磷的测定 钼酸铵分光光度法 GB 11893-1989","季度/次",8]
[31,null,null,"氟化物",10,null,"手工监测","水质 氟化物的测定 离子选择电极法（GB 7484-87）","季度/次",8]
[32,null,null,"石油类",5,null,"手工监测","水质 石油类和动植物油类的测定 红外分光光度法(HJ 637-2018)","季度/次",8]
[33,"办公楼污水处理器（DW003）","流量、水温","pH值","6.0-9.0","污水综合排放标准标准（GB 8978-1996) 表4中一级排放标准","手工监测","水质 pH值的测定 电极法 GB 1147-2020","季度/次",8]
[34,null,null,"悬浮物",70,null,"手工监测","水质 悬浮物的测定 重量法 GB 11901-1989","季度/次",8]
[35,null,null,"五日生化需氧量",20,null,"手工监测","水质 五日生化需氧量（BOD5）的测定 稀释与接种法 HJ505-2009","季度/次",8]
[36,null,null,"化学需氧量",100,null,"手工监测","水质 化学需氧量的测定  重铬酸盐法 HJ828-2017","季度/次",8]
[37,null,null,"氨氮（NH3-N）",15,null,"手工监测","水质 氨氮的测定蒸馏-中和滴定法 HJ537-2009","季度/次",8]
[38,null,null,"总磷（以P计）",0.5,null,"手工监测","水质 总磷的测定 钼酸铵分光光度法 GB 11893-1989","季度/次",8]
[39,null,null,"氟化物",10,null,"手工监测","水质 氟化物的测定 离子选择电极法（GB 7484-87）","季度/次",8]
[40,null,null,"石油类",5,null,"手工监测","水质 石油类和动植物油类的测定 红外分光光度法(HJ 637-2018)","季度/次",8]
[41,"矿山污水处理器","流量、水温","pH值","6.0-9.0","污水综合排放标准标准（GB 8978-1996) 表4中一级排放标准","手工监测","水质 pH值的测定 电极法 GB 1147-2020","季度/次",8]
[42,null,null,"悬浮物",70,null,"手工监测","水质 悬浮物的测定 重量法 GB 11901-1989","季度/次",8]
[43,null,null,"五日生化需氧量",20,null,"手工监测","水质 五日生化需氧量（BOD5）的测定 稀释与接种法 HJ505-2009","季度/次",8]
[44,null,null,"化学需氧量",100,null,"手工监测","水质 化学需氧量的测定  重铬酸盐法 HJ828-2017","季度/次",8]
[45,null,null,"氨氮（NH3-N）",15,null,"手工监测","水质 氨氮的测定蒸馏-中和滴定法 HJ537-2009","季度/次",8]
[46,null,null,"总磷（以P计）",0.5,null,"手工监测","水质 总磷的测定 钼酸铵分光光度法 GB 11893-1989","季度/次",8]
[47,null,null,"氟化物",10,null,"手工监测","水质 氟化物的测定 离子选择电极法（GB 7484-87）","季度/次",8]
[48,null,null,"石油类",5,null,"手工监测","水质 石油类和动植物油类的测定 红外分光光度法(HJ 637-2018)","季度/次",8]
[49,"主厂区雨水排放口（DW004）","流量、水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","《地表水环境质量标准》（GB3838-2002） 三类","一年/次",2]
[50,null,null,"溶解氧",5,null,"手工监测",null,"一年/次",2]
[51,null,null,"COD",20,null,"手工监测",null,"一年/次",2]
[52,null,null,"BOD5",5,null,"手工监测",null,"一年/次",2]
[53,null,null,"氨氮",1,null,"手工监测",null,"一年/次",2]
[54,null,null,"石油类",0.05,null,"手工监测",null,"一年/次",2]
[55,null,null,"Cd",0.05,null,"手工监测",null,"一年/次",2]
[56,null,null,"Hg",0.001,null,"手工监测",null,"一年/次",2]
[57,null,null,"Pb",0.05,null,"手工监测",null,"一年/次",2]
[58,null,null,"粪大肠菌群",10000,null,"手工监测",null,"一年/次",2]
[59,"矿山矿区外排水","流量、水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","《地表水环境质量标准》（GB3838-2002） 三类","一年/次",2]
[60,null,null,"溶解氧",5,null,"手工监测",null,"一年/次",2]
[61,null,null,"COD",20,null,"手工监测",null,"一年/次",2]
[62,null,null,"BOD5",5,null,"手工监测",null,"一年/次",2]
[63,null,null,"氨氮",1,null,"手工监测",null,"一年/次",2]
[64,null,null,"石油类",0.05,null,"手工监测",null,"一年/次",2]
[65,null,null,"Cd",0.05,null,"手工监测",null,"一年/次",2]
[66,null,null,"Hg",0.001,null,"手工监测",null,"一年/次",2]
[67,null,null,"Pb",0.05,null,"手工监测",null,"一年/次",2]
[68,null,null,"粪大肠菌群",10000,null,"手工监测",null,"一年/次",2]
[]
["梁平海创2022年-2023年环境自行监测方案（地下水）"]
["序号","监测位置","监测介质","监测方式","监测指标","限值(mg/L)","监测方式","监测依据及方法","监测频次"]
[1,"厂区下游","地下水（潜水含水层，地下水位以下1.0米左右）","手工监测","PH","6.5-8.5","手工监测","水质 pH值的测定 电极法 GB 1147-2020","1次/年"]
[2,null,null,"手工监测","砷",0.01,"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（6.1氢化物原子荧光法）","1次/年"]
[3,null,null,"手工监测","氨氮",0.5,"手工监测","水质 氨氮的测定纳氏试剂分光光度法 HJ535-2009","1次/年"]
[4,null,null,"手工监测","汞",0.001,"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（8.1原子荧光法）","1次/年"]
[5,null,null,"手工监测","铬（六价）",0.05,"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（10铬（六价）10.1分光光度法）","1次/年"]
[6,null,null,"手工监测","镉",0.005,"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（9.1无火焰原子吸收分光光度法）","1次/年"]
[7,null,null,"手工监测","铜",0.005,"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（1.4电感耦合等离子体发射光谱法）","1次/年"]
[8,null,null,"手工监测","锌",{"v":1,"d":"1.0"},"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（1.4电感耦合等离子体发射光谱法）","1次/年"]
[9,null,null,"手工监测","铅",{"v":0.01,"d":"0.0"},"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（11.1无火焰原子吸收分光光度法）","1次/年"]
[10,null,null,"手工监测","镍",{"v":1,"d":"1.0"},"手工监测","生活引用岁标准检验方法 金属指标 GB/T5750.6-2006（1.4电感耦合等离子体发射光谱法）","1次/年"]

{"sheet":"周边环境质量（海创）","index":5,"n_rows":48,"n_cols":9,"rows_kept":48,"merged":[[0,0,0,8],[2,0,17,0],[2,1,17,1],[2,2,17,2],[2,3,17,3],[5,6,6,6],[7,6,9,6],[11,6,16,6],[18,0,33,0],[18,1,33,1],[18,2,33,2],[18,3,32,3],[21,6,22,6],[23,6,25,6],[27,6,32,6],[34,0,47,0],[34,1,47,1],[34,2,47,2],[34,3,47,3]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（周边环境质量）"]
["序号","监测位置","监测介质","监测方式","监测指标","手工监测频次","监测依据及方法","两年监测次数","备注"]
[1,"固废储存库附近","土壤","手工监测","pH","1次/年","土壤  pH值的测定  电位法 HJ 962-2018",2,"梁平海创"]
[{"$nulls":4},"汞","1次/年","土壤质量 总汞、总砷、总铅的测定 原子荧光法  第1部分：土壤中总汞的测定 GB/T 22105.1-2008",2,"梁平海创"]
[{"$nulls":4},"砷","1次/年","土壤质量 总汞、总砷、总铅的测定 原子荧光法第2部分：土壤中总砷的测定 GB/T 22105.2-2008",2,"梁平海创"]
[{"$nulls":4},"镉","1次/年","土壤质量 铅、镉的测定 石墨炉原子吸收分光光度法 GB/T 17141-1997",2,"梁平海创"]
[{"$nulls":4},"铅","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铜","1次/年","土壤和沉积物 铜、锌、铅、镍、铬的测定 火焰原子吸收分光光度法 HJ 491-2019",2,"梁平海创"]
[{"$nulls":4},"镍","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铬","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"锰","1次/年","土壤和沉积物 12种金属元素的测定 王水提取-电感耦合等离子体质谱法 HJ 803-2016",2,"梁平海创"]
[{"$nulls":4},"铍","1次/年","《全国土壤污染状况详查土壤样品分析测试方法技术规定》（环办土壤函﹝2017﹞1625号）（第一部分土壤样品无机项目分析测试方法  2-2 电感耦合等离子体发射光谱法）",2,"梁平海创"]
[{"$nulls":4},"锡","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"锑","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"钴","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铊","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"钒","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"二噁英","1次/年",null,2,"梁平海创"]
[2,"蓝家湾","土壤","手工监测","pH","1次/年","土壤  pH值的测定  电位法 HJ 962-2018",2,"梁平海创"]
[{"$nulls":4},"汞","1次/年","土壤质量 总汞、总砷、总铅的测定 原子荧光法  第1部分：土壤中总汞的测定 GB/T 22105.1-2008",2,"梁平海创"]
[{"$nulls":4},"砷","1次/年","土壤质量 总汞、总砷、总铅的测定 原子荧光法第2部分：土壤中总砷的测定 GB/T 22105.2-2008",2,"梁平海创"]
[{"$nulls":4},"镉","1次/年","土壤质量 铅、镉的测定 石墨炉原子吸收分光光度法 GB/T 17141-1997",2,"梁平海创"]
[{"$nulls":4},"铅","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铜","1次/年","土壤和沉积物 铜、锌、铅、镍、铬的测定 火焰原子吸收分光光度法 HJ 491-2019",2,"梁平海创"]
[{"$nulls":4},"镍","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铬","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"锰","1次/年","土壤和沉积物 12种金属元素的测定 王水提取-电感耦合等离子体质谱法 HJ 803-2016",2,"梁平海创"]
[{"$nulls":4},"铍","1次/年","《全国土壤污染状况详查土壤样品分析测试方法技术规定》（环办土壤函﹝2017﹞1625号）（第一部分土壤样品无机项目分析测试方法  2-2 电感耦合等离子体发射光谱法）",2,"梁平海创"]
[{"$nulls":4},"锡","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"锑","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"钴","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"铊","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"钒","1次/年",null,2,"梁平海创"]
[{"$nulls":4},"二噁英","1次/年",null,2,"梁平海创"]
[3,"安居社区（搬迁安置点）","环境空气","手工监测","SO2","1次/年","环境空气 二氧化硫的测定  甲醛吸收-副玫瑰苯胺分光光度法及修改单HJ 482-2009",2,"梁平海创"]
[{"$nulls":4},"NO2","1次/年","环境空气 氮氧化物（一氧化氮和二氧化氮）的测定  盐酸萘乙二胺分光光度法及修改单HJ479-2009",2]
[{"$nulls":4},"PM10","1次/年","环境空气PM10和PM2.5的测定  重量法及修改单HJ618-2011",2]
[{"$nulls":4},"PM2.5","1次/年","环境空气PM10和PM2.5的测定  重量法及修改单HJ618-2011",2]
[{"$nulls":4},"氟化物","1次/年","环境空气  氟化物的测定  滤膜采样/氟离子选择电极法HJ955-2018",2]
[{"$nulls":4},"HCl","1次/年",null,2]
[{"$nulls":4},"H2S","1次/年",null,2]
[{"$nulls":4},"NH3","1次/年",null,2]
[{"$nulls":4},"铬（六价）","1次/年",null,2]
[{"$nulls":4},"Hg","1次/年",null,2]
[{"$nulls":4},"Pb（铅）","1次/年","空气和废气颗粒物中 铅等金属元素的测定 电感耦合等离子体质谱法 HJ657-20113",2]
[{"$nulls":4},"Cd（镉）","1次/年","空气和废气颗粒物中 铅等金属元素的测定 电感耦合等离子体质谱法 HJ657-20113",2]
[{"$nulls":4},"As（砷）","1次/年","空气和废气颗粒物中 铅等金属元素的测定 电感耦合等离子体质谱法 HJ657-20113",2]
[{"$nulls":4},"二噁英","1次/年",null,2,"梁平海创"]

{"sheet":"比对监测","index":6,"n_rows":16,"n_cols":13,"rows_kept":16,"merged":[[0,0,0,12],[2,0,9,0],[2,1,9,1],[2,2,9,2],[2,4,4,4],[2,5,4,5],[2,8,5,8],[2,9,4,9],[6,4,8,4],[6,5,8,5],[6,6,8,6],[6,8,8,8],[10,0,15,0],[10,1,15,1],[10,2,15,2],[10,4,12,4],[10,5,12,5],[10,8,14,8],[10,9,12,9]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（比对监测）"]
["序号","在线设备","排口代码","参数","型号","厂家","产品编号","量程范围","监测采样要求","监测依据及方法","比对频次","两年监测次数","备注"]
[1,"窑尾在线监测","DA076","流速","PT-1D","重庆川仪分析仪器有限公司",2004070405,"0-40m/s","一个生产周期内比对5组数据对","固定污染源排气中 颗粒物测定与气态污染物采样方法GB/T 16157-1996 ","季度/次",8]
[{"$nulls":3},"温度",null,null,140589,"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"压力",null,null,"/","（-4-4）KPa",null,null,"季度/次",8]
[{"$nulls":3},"颗粒物","DT600","重庆川仪分析仪器有限公司","PD071364","0-200mg/m3",null,"固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"二氧化硫","PA200-UV","重庆川仪分析仪器有限公司","CY2015037","0-500mg/m3","一个生产周期内比对9组数据对"," 固定污染源废气 二氧化硫的测定 便携式紫外吸收法（HJ 1131-2020） ","季度/次",8]
[{"$nulls":3},"氮氧化物",{"$nulls":3},"0-1000mg/m3",null," 固定污染源废气  氮氧化物的测定 便携式紫外吸收法（HJ 1132-2020）","季度/次",8]
[{"$nulls":3},"氧含量",{"$nulls":3},"0-25%",null,"《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）（5.2.6.3电化学法测定氧（B)）","季度/次",8]
[{"$nulls":3},"湿度","HMS545C","南京埃森环境技术有限公司",20151432,"0-40%","一个生产周期内比对5组数据对","\n固定污染源排气中 颗粒物测定与气态污染物采样方法GB/T 16157-1996 ","季度/次",8]
[2,"窑头在线监测","DA067","流速","PT-1D","重庆川仪分析仪器有限公司",2004070406,"0-40m/s","一个生产周期内比对5组数据对","固定污染源排气中 颗粒物测定与气态污染物采样方法GB/T 16157-1996 ","季度/次",8]
[{"$nulls":3},"温度",null,null,"/","（-4-4）KPa",null,null,"季度/次",8]
[{"$nulls":3},"压力",null,null,140588,"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"颗粒物","DT600","重庆川仪分析仪器有限公司","PD071364","0-200mg/m3",null,"固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"湿度","KC-545","重庆创辉科技有限公司","CH/Q-PT-GA180066","0-40%",null,"\n固定污染源排气中 颗粒物测定与气态污染物采样方法GB/T 16157-1996 ","季度/次",8]
[{"$nulls":3},"氧含量","ZQ-12B(Q)","重庆创辉科技有限公司","CH/Q-PT-GA180073","0-25%","一个生产周期内比对9组数据对","《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）（5.2.6.3电化学法测定氧（B)）","季度/次",8]

{"sheet":"油烟监测","index":7,"n_rows":8,"n_cols":12,"rows_kept":8,"merged":[[0,0,0,11],[2,1,4,1],[2,2,4,2],[5,1,7,1],[5,2,7,2]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（油烟监测）"]
["序号","监测位置","监测内容","污染物名称","限值(mg/m3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[1,"专家公寓食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[2,null,null,"非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[3,null,null,"臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]
[4,"员工大食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[5,null,null,"非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[6,null,null,"臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]

{"sheet":"个人剂量监测","index":8,"n_rows":4,"n_cols":10,"rows_kept":4,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（个人剂量监测）"]
["序号","监测位置","检测项目","姓名","检测/评价依据","检测方法","监测频次","职业类型","两年检测次数","备注"]
[1,"/","外照射个人剂量监测","潘川","GBZ128-2019 GB18871-2002","热释光个人剂量监测","一季度/次","工业探伤（3B）",8]
[2,"/","外照射个人剂量监测","敬希强","GBZ128-2019 GB18871-2002","热释光个人剂量监测","一季度/次","工业探伤（3B）",8]

{"sheet":"皮带探伤设备辐射检测","index":9,"n_rows":4,"n_cols":10,"rows_kept":4,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["梁平海螺2024年-2025年环境自行监测方案（场所辐射环境监测）"]
["序号","受检设备名称","监测位置描述","监测项目","监测方法","监测方式","监测频次","监测评价依据","两年监测次数","备注"]
[1,"矿用输送带钢丝绳芯无损探伤装置","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","一年/次","《工业探伤放射防护要求标准》GBZ117-2022 ",2]
[2,"石灰石在线分析仪/DF-5701（YQ101S01RY09067）","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","一年/次","GBZ125-2009《含密封源仪表的放射卫生防护要求》",2]