{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["废气有组织","废气无组织","厂界噪声","废水","周边环境质量","比对监测","油烟监测","个人剂量监测","场所辐射环境监测"],"not_rendered":{"external_links":1,"defined_names":12,"comments":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气有组织","index":0,"n_rows":310,"n_cols":18,"rows_kept":310,"merged":[[0,0,0,17],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[1,8,3,8],[1,9,3,9],[1,10,3,10],[1,11,3,11],[1,12,3,12],[1,13,3,13],[1,14,3,14],[1,15,3,15],[1,16,3,16],[1,17,3,17],[18,0,24,0],[18,1,24,1],[18,2,24,2],[18,3,24,3],[18,4,24,4],[18,6,24,6],[18,7,24,7],[18,8,24,8],[18,9,24,9],[39,0,45,0],[39,1,45,1],[39,2,45,2],[39,3,45,3],[39,4,45,4],[39,6,45,6],[39,7,45,7],[39,8,45,8],[39,9,45,9],[55,0,66,0],[55,1,66,1],[55,2,66,2],[55,3,66,3],[55,4,66,4],[55,6,66,6],[55,7,66,7],[55,8,66,8],[55,9,66,9],[97,0,100,0],[97,1,100,1],[97,2,100,2],[97,3,100,3],[97,4,100,4],[97,6,100,6],[97,7,100,7],[97,8,100,8],[97,9,100,9],[282,0,284,0],[282,1,284,1],[282,2,284,2],[282,3,284,3],[282,4,284,4],[285,0,289,0],[285,1,289,1],[285,2,289,2],[285,3,289,3],[285,4,289,4],[297,0,297,17],[298,0,303,0],[298,1,303,1],[298,2,303,2],[298,3,303,3],[298,6,303,6],[298,7,303,7],[298,8,303,8],[298,9,303,9],[304,0,309,0],[304,1,309,1],[304,2,309,2],[304,3,309,3],[304,6,309,6],[304,7,309,7],[304,8,309,8],[304,9,309,9]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（有组织废气）"]
["序号","污染治理设施名称","设备型号","排口编号","监测内容","污染物","设计处理风量   （Nm3/h)","排气筒高度(m)","排气筒出口内径(m)","排口类型","限值(mg/m3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[]
[]
[1,"二期破碎机袋收尘器","HMC-96","DA001","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",26800,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[2,"3#带尾部袋收尘器","JQM6×32","DA002","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[3,"二期4-1#带尾部袋收尘器","JQM5×32","DA003","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,16,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[4,"2#带尾部袋收尘器","JQM6×32","DA004","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[5,"一期4#带尾部袋收尘器","JQM6×32","DA005","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[6,"二期0#带尾部袋收尘器","JQM5×32","DA006","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[7,"反击式破碎机出料皮带收尘器","JQM5×32","DA007","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",22207,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[8,"粘土破碎机出料皮带收尘器","JQM5×32","DA008","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",22207,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[9,"1136皮带收尘器","JQM4×32","DA009","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[10,"1139皮带收尘器","JQM4×32","DA010","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,18,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[11,"1#石灰石库顶收尘器","JQM4×32","DA011","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,30,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[12,"1#线均化库顶袋除尘器","JQM4×64","DA012","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17800,66,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[13,"1#线均化库底袋除尘器","JQM5×32","DA013","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[14,"主厂区熟料1#大库顶收尘器","JQM5×96","DA014","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",33500,43,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[15,"1#线窑尾收尘器","CBMP240-2-2×4","DA015","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",760000,90,6,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"二氧化硫",{"$nulls":4},200,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 二氧化硫的测定 非分散红外吸收法HJ 629-2011",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"氮氧化物",{"$nulls":4},350,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 氮氧化物的测定 非分散红外吸收法HJ 692-2014",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"氟化物",{"$nulls":4},5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",4]
[{"$nulls":5},"汞及其化合物",{"$nulls":4},0.05,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","5.3.7.2原子荧光分光光度法",4]
[{"$nulls":5},"二噁英类",{"$nulls":4},"0.1ngTEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","年/次","非连续采样至少3个样","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱-高分辨质谱法HJ/T 77.2-2008",2]
[{"$nulls":5},"氨（氨气）",{"$nulls":4},10,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 次氯酸钠-水杨酸分光光度法 HJ 534-2009",8]
[16,"1#/2#煤磨主收尘器","PPC128-2×5M","DA016","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","90000-110000",37,2,"一般排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[17,"1#窑头收尘器","CBMP378-2×4","DA017","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",580000,40,3.7,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[18,"出一期石灰石堆场1#转运站收尘器","JQM5×32","DA018","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[19,"出一期石灰石堆场2#转运站收尘器","JQM5×32","DA019","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[20,"一线混料皮带头部收尘器","JQM3×32","DA020","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6900,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[21,"出原煤堆场1#皮带收尘器","LPF(M)5×32","DA021","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[22,"入原煤堆场皮带袋收尘器","LPF(M)5×32","DA022","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[23,"原煤2#皮带头部收尘器","LPF(M)5×32","DA023","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,20,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[24,"1#煤粉仓收尘器","LPF(M)4×32 ","DA024","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,39,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[25,"1#原料磨生料输送斜槽收尘器","PMD-10B","DA025","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",7200,16,"0.32（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[26,"2#石灰石库顶袋收尘器","JQM4×32","DA026","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,30,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[27,"2#均化库顶袋收尘器","JQM4×64","DA027","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17800,66,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[28,"2#均化库底袋收尘器","JQM5×32","DA028","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[29,"主厂区熟料2#大库收尘器","JQM5×96","DA029","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",33500,43,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[30,"2#窑尾收尘","CBMP240-2-2×4","DA030","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",760000,90,6,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"二氧化硫",{"$nulls":4},200,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 二氧化硫的测定 非分散红外吸收法HJ 629-2011",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"氮氧化物",{"$nulls":4},350,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 氮氧化物的测定 非分散红外吸收法HJ 692-2014",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"氟化物",{"$nulls":4},5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",4]
[{"$nulls":5},"汞及其化合物",{"$nulls":4},0.05,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","5.3.7.2原子荧光分光光度法",4]
[{"$nulls":5},"二噁英类",{"$nulls":4},"0.1ngTEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","年/次","非连续采样至少3个样","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱-高分辨质谱法HJ/T 77.2-2008",2]
[{"$nulls":5},"氨（氨气）",{"$nulls":4},10,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 次氯酸钠-水杨酸分光光度法 HJ 534-2009",8]
[31,"2#煤粉仓收尘器","LPF(M)4×32 ","DA031","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,30,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[32,"2#窑头收尘器","CBMP378-2×4","DA032","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",580000,40,3.7,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[33,"二线混料皮带尾部袋收尘器","JQM4×32","DA033","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[34,"二线混料皮带头部袋收尘器","JQM4×32","DA034","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[35,"2#原料磨生料输送斜槽收尘器","PMD-10B","DA035","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",7200,16,0.35,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[36,"3#石子库袋收尘器","JQM4×32","DA036","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,35,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[37,"3#线均化库顶袋收尘器","JQM6×32","DA037","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,66,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[38,"3#线均化库底袋收尘器","JQM5×32","DA038","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[39,"主厂区熟料3#大库顶收尘器","JQM5×96","DA039","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",33500,43,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[40,"3#窑尾收尘器","CBMP252-2-2×4","DA040","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",785000,90,5.6,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"二氧化硫",{"$nulls":4},200,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 二氧化硫的测定 非分散红外吸收法HJ 629-2011",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"氮氧化物",{"$nulls":4},350,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气 氮氧化物的测定 非分散红外吸收法HJ 692-2014",8,"季度监测时，在委托报告上体现监测数据"]
[{"$nulls":5},"汞及其化合物",{"$nulls":4},0.05,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",4]
[{"$nulls":5},"氟化物",{"$nulls":4},5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","5.3.7.2原子荧光分光光度法",4]
[{"$nulls":5},"氨（氨气）",{"$nulls":4},10,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 氨的测定 次氯酸钠-水杨酸分光光度法 HJ 534-2009",8]
[{"$nulls":5},"氯化氢（HCl)",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","半年/次","非连续采样至少3个样","环境空气和废气 氯化氢的测定 离子色谱法HJ 549-2016代替HJ 549-2009",4]
[{"$nulls":5},"氟化氢（HF)",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","半年/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",4]
[{"$nulls":5},"铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物",{"$nulls":4},0.5,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","半年/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",4]
[{"$nulls":5},"铊、镉、铅、砷及其化合物",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","半年/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",4]
[{"$nulls":5},"总有机碳",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","半年/次","非连续采样至少3个样","环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017",4]
[{"$nulls":5},"二噁英类",{"$nulls":4},"0.1ngTEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","年/次","非连续采样至少3个样","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱-高分辨质谱法HJ/T 77.2-2008",2]
[41,"3#煤磨主收尘器","PPC128-2×5M","DA041","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","90000-110000",37,1.4,"一般排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[42,"3#窑头收尘器","CBMP378-2×4","DA042","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",580000,40,3.8,"主要排放口",30,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","自动监测","在线监测发生故障时，4次/日，间隔不超过6小时","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",8,"季度监测时，在委托报告上体现监测数据"]
[43,"出二期石灰石堆场1#转运站收尘器","JQM4×32","DA043","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[44,"出二期石灰石堆场2#转运站收尘器","JQM4×32","DA044","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[45,"三线混料皮带头部袋除尘器","JQM4×32","DA045","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[46,"3#入原料磨皮带尾部袋收尘器","JQM4×32","DA046","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[47,"3#煤粉仓收尘器","LPF(M)4×32","DA047","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,37,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[48,"入3#煤磨皮带收尘器","LPF(M)5×32","DA048","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[49,"3#原料磨生料输送斜槽袋收尘器","JQM3×32","DA049","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6900,16,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[50,"钢渣皮带1#收尘器","JQM3×32","DA050","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6900,15,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[51,"钢渣转运站皮带2#收尘器","JQM3×32","DA051","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6900,15,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[52,"灰仓袋收尘器","LQMC-48-F","DA052","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",4000,23,"0.25（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[53,"不然物仓袋收尘器","DMD-80","DA053","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",4320,15,"0.25（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[54,"3075皮带尾部收尘器器","FMD5×32","DA054","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,23,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[55,"1#粉煤灰库顶收尘器","LFGM32-4","DA055","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,27,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[56,"1#水泥库顶收尘器","LFGM32-5","DA056","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[57,"1#水泥库底收尘器","LFGM32-6","DA057","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[58,"2#水泥库顶收尘器","LFGM32-6","DA058","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[59,"2#水泥库底收尘器","LFGM32-6","DA059","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[60,"1964汽散仓顶收尘器","LFGM32-4","DA060","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[61,"3万3熟料1号库顶收尘器","LFGM32-6","DA061","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,29,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[62,"熟料发散库1号库顶收尘器","LFGM32-5","DA062","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[63,"堆场石膏破碎机收尘器","LFGM32-4","DA063","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[64,"石灰石出库皮带中部收尘器","LFGM32-4","DA064","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[65,"1#水泥磨尾袋收尘器","PPCA96-8L","DA065","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",53000,35,1.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[66,"1#水泥磨主袋收尘器","PPCA128-2*13","DA066","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",240000,30,2.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[67,"1#包装机主收尘器","LFGM64-5","DA067","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17856,21,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[68,"1#包装机副收尘器","LFGM32-4","DA068","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,24,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[69,"2#包装机主收尘器","LFGM64-5","DA069","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17856,21,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[70,"2#包装机副收尘器","LFGM32-4","DA070","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,24,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4,"合理安排监测计划，保证每个季度相同种类治理设施的监测点位数量基本平均分布"]
[71,"生活垃圾贮存除臭系统排放口","4-72No.8C","DA071","烟气流速,烟气温度,烟气含湿量,烟道截面积","臭气浓度",30000,25,1,"一般排放口","/","恶臭污染物排放标准（GB14554-93）","手工监测","半年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",4]
[{"$nulls":5},"硫化氢",{"$nulls":4},"/","恶臭污染物排放标准（GB14554-93）","手工监测","半年/次","非连续采样至少3个样","5.4.10.3亚甲基蓝分光光度法（B)",4]
[{"$nulls":5},"氨（氨气）",{"$nulls":4},10,"恶臭污染物排放标准（GB14554-93）","手工监测","半年/次","非连续采样至少3个样","环境空气 氨的测定 次氯酸钠-水杨酸分光光度法 HJ 534-2009",4]
[{"$nulls":5},"颗粒物",{"$nulls":4},20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","固定污染源废气低浓度颗粒物的测定重量法HJ 836-2017",4]
[72,"骨料3092皮带头部收尘器","FMD5×32","DA072","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[73,"汽散熟料收尘器","LFGM32-5","DA073","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[74,"1954斗提船散收尘器","HMC-64","DA074","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[75,"4#水泥库旁船包斜槽收尘器","HMC-64","DA075","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[76,"1954斗提汽散斜槽收尘器","HMC-64","DA076","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[77,"一期成品斜槽尾部收尘器","HMC-96","DA077","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[78,"一期成品斜槽中部收尘器","HMC-96","DA078","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[79,"一期成品斜槽头部收尘器","HMC-96","DA079","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[80,"1043头部收尘器","LFGM32-4","DA080","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[81,"1044头部收尘器","LFGM32-4","DA081","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[82,"石灰石库顶收尘器","LFGM32-4","DA082","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,28,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[83,"1763尾部2#收尘器","FMD32-5","DA083","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[84,"石灰石出库皮带头部收尘器","LFGM32-4","DA084","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[85,"1#除泥收尘器","CD6D","DA085","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",28000,15,0.65,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[86,"2#除泥收尘器","FMD5×96A","DA086","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","27900-33480",15,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[87,"4#泊位1#装船机收尘器","CDD-800","DA087","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",43000,15,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[88,"1706尾部收尘器","LFGM32-5","DA088","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[89,"1706头部收尘器","LFGM32-5","DA089","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[90,"1707尾部收尘器","LFGM32-5","DA090","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[91,"1707头部收尘器","LFGM32-5","DA091","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[92,"1708尾部收尘器","LFGM32-5","DA092","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[93,"1708头部收尘器","LFGM32-5","DA093","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[94,"三号转运站收尘器","LFGM32-4","DA094","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[95,"1739头部平台收尘器","LFGM32-5","DA095","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[96,"1739中部收尘器","LFGM32-5","DA096","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[97,"1739尾部收尘器","LFGM32-5","DA097","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[98,"1740头部平台收尘器","LFGM32-5","DA098","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[99,"1740中部收尘器","LFGM32-5","DA099","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[100,"1740尾部收尘器","LFGM32-5","DA100","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[101,"1764尾部收尘器","LFGM32-5","DA101","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[102,"1751头部收尘器","LFGM32-4","DA102","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[103,"1102头部收尘器","LFGM32-4","DA103","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[104,"1104头部收尘器","LFGM32-4","DA104","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[105,"1105头部收尘器","LFGM32-4","DA105","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[106,"一级筛分机收尘器","FMD5×96A","DA106","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","27900-33480",15,0.75,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[107,"一期辅材仓收尘器","LFGM32-4","DA107","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[108,"一期熟料仓收尘器","LFGM32-4","DA108","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[109,"1#水泥磨喂料皮带收尘器","LFGM32-5","DA109","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[110,"1749转运站收尘器","LFGM32-4","DA110","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[111,"2#粉煤灰库顶收尘器","LFGM32-4","DA111","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,27,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[112,"3#水泥库顶收尘器","LFGM32-5","DA112","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[113,"3#水泥库底收尘器","LFGM32-6","DA113","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[114,"2#水泥磨尾袋收尘器","PPCA96-8L","DA114","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",53000,35,1.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[115,"3#包装机主收尘器","LFGM64-5","DA115","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17856,21,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[116,"3#包装机副收尘器","LFGM32-4","DA116","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,24,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[117,"2#水泥磨主袋收尘器","PPCA128-2*13","DA117","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",240000,30,2.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[118,"1763头部2#收尘器","FMD32-5","DA118","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[119,"1962斗提尾部收尘器","HMC-64","DA119","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[120,"2706尾部收尘器","LFGM32-5","DA120","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[121,"2706头部收尘器","LFGM32-5","DA121","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[122,"2707头部收尘器","LFGM32-5","DA122","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[123,"2707尾部收尘器","LFGM32-5","DA123","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[124,"2708尾部收尘器","LFGM32-5","DA124","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[125,"2708头部收尘器","LFGM32-5","DA125","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[126,"2716头部收尘器","LFGM32-5","DA126","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[127,"2#水泥磨喂料皮带收尘器","LFGM32-5","DA127","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[128,"3#粉煤灰库顶收尘器","LFGM32-4","DA128","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,27,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[129,"4#水泥库顶收尘器","LFGM32-5","DA129","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[130,"4#水泥库底收尘器","LFGM32-6","DA130","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[131,"5#水泥库顶收尘器","LFGM32-5","DA131","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[132,"5#水泥库底收尘器","LFGM32-6","DA132","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[133,"3万3熟料2号库顶收尘器","LFGM32-6","DA133","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,29,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[134,"熟料发散库2号库顶收尘器","LFGM32-5","DA134","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[135,"3#水泥磨尾袋收尘器","PPCA96-8L","DA135","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",53000,35,1.35,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[136,"3#水泥磨主袋收尘器","PPCA128-2*13","DA136","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",240000,30,2.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[137,"4#包装机主收尘器","LFGM64-5","DA137","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17856,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[138,"4#包装机副收尘器","LFGM32-4","DA138","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[139,"4#包装机小收尘器","HMC-64","DA139","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.4（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[140,"1#泊位1#门吊收尘器","FMD4×64-A","DA140","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17800,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[141,"3074皮带尾部收尘器","FMD5×32","DA141","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,18,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[142,"2954斗提船散收尘器","HMC-64","DA142","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[143,"2954斗提汽散斜槽收尘器","HMC-64","DA143","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[144,"二期成品斜槽尾部收尘器","HMC-96","DA144","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[145,"二期成品斜槽中部收尘器","HMC-96","DA145","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[146,"二期成品斜槽头部收尘器","HMC-96","DA146","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[147,"3706头部收尘器","FMD5×32","DA147","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",9300,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[148,"3707头部收尘器","FMD5×32","DA148","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",9300,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[149,"3708头部收尘器","FMD5×32","DA149","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",9300,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[150,"3716头部收尘器","FMD4×32","DA150","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[151,"3718头部收尘器","FMD5×32","DA151","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",9300,16,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[152,"1741头部平台收尘器","LFGM32-5","DA152","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[153,"1741中部收尘器","LFGM32-5","DA153","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[154,"1741尾部收尘器","LFGM32-5","DA154","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[155,"二期辅材仓收尘器","LFGM32-4","DA155","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[156,"二期熟料仓收尘器","LFGM32-4","DA156","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,25,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[157,"3#水泥磨喂料皮带收尘器","LFGM32-5","DA157","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[158,"4#粉煤灰库顶收尘器","LFGM32-4","DA158","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,27,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[159,"6#水泥库顶收尘器","LFGM32-5","DA159","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,38,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[160,"6#水泥库底收尘器","LFGM32-6","DA160","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11160,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[161,"4#水泥磨尾袋收尘器","PPCA96-8L","DA161","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",53000,35,1.35,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[162,"4#水泥磨主袋收尘器","PPCA128-2*13","DA162","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",240000,30,2.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[163,"5#包装机主收尘器","LFGM64-5","DA163","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17856,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[164,"5#包装机副收尘器","LFGM32-4","DA164","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",4]
[165,"5#包装机小收尘器","HMC-64","DA165","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.4（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[166,"3071皮带中部收尘器","FMD5×32","DA166","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,23,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[167,"2954斗提顶部入船散斜槽收尘器","HMC-64","DA167","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",15,"0.2(方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[168,"4#水泥磨喂料皮带收尘器","LFGM32-5","DA168","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[169,"39641船散仓顶收尘器","LFGM32-4","DA169","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[170,"39642船散仓顶收尘器","LFGM32-4","DA170","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[171,"1#泊位2#门吊收尘器","FMD4×64-A","DA171","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",17800,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[172,"5#装船机收尘器","DMC-156","DA172","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",32130,15,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[173,"7#装船机收尘器","DMC-182","DA173","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",38400,15,1,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[174,"1767尾部转运站收尘器","LFGM32-5","DA174","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,27,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[175,"3#泊位1762皮带尾部收尘器","LFGM32-5","DA175","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8928,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[176,"1763头部收尘器","LFGM32-4","DA176","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,22,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[177,"1763尾部收尘器","LFGM32-4","DA177","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[178,"1765尾部收尘器","LFGM32-4","DA178","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,22,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[179,"1765头部收尘器","LFGM32-4","DA179","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[180,"古池坝袋收尘器","JQM6×32","DA180","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.2,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[181,"廖山袋收尘器","JQM6×32","DA181","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,18,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[182,"大房沟袋收尘器","JQM6×32","DA182","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[183,"4#泊位2#装船机收尘器","CDD-800","DA183","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",43000,15,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[184,"一期破碎机袋收尘器","HMC-96","DA184","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",26800,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[185,"一期0#带尾部袋收尘器","LFCM5×32","DA185","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,16,"0.45（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[186,"2954斗提顶部入汽散斜槽收尘器","HMC-64","DA186","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","2900-4300",30,"0.2(方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[187,"二期4-2#带尾部袋收尘器","JQM5×32","DA187","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[188,"二级筛分机收尘器","FMD5×96A","DA188","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","27900-33480",15,0.75,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[189,"骨料石子库顶收尘器","FMD5×64B","DA189","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",22300,35,0.7,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[190,"1#、2#成品库收尘器","FMD5×32","DA190","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,23,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[191,"4#包装机2#副收尘器","DMD96A","DA191","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",15,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[192,"船散仓收尘器","DMD96A","DA192","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",15,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[193,"船包收尘器","DMD96A","DA193","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5200-7000",15,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[194,"1102尾部收尘器","LFGM32-4","DA194","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[195,"5#泊位装船机收尘器","CD6D","DA195","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",28000,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[196,"3#、4#成品库收尘器","FMD5×32","DA196","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,23,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[197,"骨料1#发散库顶收尘器","FMD5×32","DA197","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,30,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[198,"骨料3091皮带头部收尘器","DMD80A","DA198","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","4000-6000",15,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[199,"骨料2#发散库顶收尘器","FMD5×32","DA199","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,30,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[200,"骨料3091皮带中部收尘器","FMD5×32","DA200","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[201,"骨料3#发散库顶收尘器","FMD5×32","DA201","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,30,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[202,"骨料3091皮带尾部收尘器","FMD5×32","DA202","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[203,"入石子库转运站收尘器","FMD5×32","DA203","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,20,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[204,"石子库底1#收尘器","FMD6×32","DA204","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[205,"石子库底2#收尘器","FMD6×32","DA205","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[206,"3051长皮带尾部收尘器","FMD5×32","DA206","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[207,"3019回渣皮带收尘器","FMD5×32","DA207","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[208,"3021入矿山回渣皮带收尘器","FMD5×32","DA208","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[209,"3052长皮带尾部收尘器","FMD5×32","DA209","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,19,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[210,"3053皮带尾部收尘器","FMD5×32","DA210","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,23,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[211,"4#泊位3191皮带尾部收尘器","DMD80A","DA211","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",3600,15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[212,"4#泊位3191皮带中部收尘器","FMD5×32","DA212","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[213,"4#泊位3191皮带头部收尘器","FMD5×32","DA213","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[214,"4#泊位3192皮带头部收尘器","FMD6×32","DA214","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[215,"4#泊位3193皮带头部收尘器","FMD6×32","DA215","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[216,"4#泊位3194皮带头部收尘器","CDD-550","DA216","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",29000,15,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[217,"三期粉磨站入B磨转运站皮带头部收尘器","FMD32-4","DA217","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,30,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[218,"4#泊位3190皮带头部收尘器","LFGM32-4","DA218","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",6696,15,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[219,"骨料汽散发运收尘器","FMD5-96A","DA219","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",27000,15,0.75,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[220,"三期粉磨站B磨循环斗提收尘器","FMD32-5","DA220","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,37,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[221,"三期粉磨站出堆场皮带头部收尘器","FMD32-4","DA221","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,30,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[222,"三期粉磨站石灰石中转皮带收尘器","FMD32-4","DA222","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,25,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[223,"三期粉磨站A磨循环斗提收尘器","FMD32-5","DA223","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,37,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[224,"三期粉磨站A磨熟料出库皮带收尘器","FMD32-6","DA224","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[225,"三期粉磨站混合材2#皮带收尘器","FMD32-4","DA225","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,28,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[226,"三期粉磨站熟料出库中转站收尘器","FMD32-6","DA226","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,18,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[227,"三期粉磨站入A磨转运站皮带头部收尘器","FMD32-4","DA227","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,30,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[228,"三期粉磨站B磨熟料出库皮带收尘器","FMD32-6","DA228","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[229,"三期粉磨站混合材1#皮带收尘器","FMD32-4","DA229","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,25,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[230,"三期粉磨站辅材仓顶收尘器","FMD32-4","DA230","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,25,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[231,"三期粉磨站B磨主袋收尘器","DMC633-2*11","DA231","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",660000,37,2.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[232,"三期粉磨站A磨主袋收尘器","DMC633-2*11","DA232","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",660000,37,2.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",8]
[233,"三期粉磨站石灰石库顶收尘器","FMD32-4","DA233","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,40,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[234,"三期粉磨站2#熟料库顶收尘器","FMD32-4","DA234","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8900,50,0.45,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[235,"三期粉磨站1#熟料库顶收尘器","FMD32-6","DA235","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,50,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[236,"三期粉磨站6#水泥库顶收尘器","FMD32-5","DA236","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[237,"三期粉磨站6#水泥库底收尘器","FMD32-6","DA237","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[238,"三期粉磨站2#水泥库顶收尘器","FMD32-5","DA238","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[239,"三期粉磨站2#水泥库底收尘器","FMD32-6","DA239","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[240,"三期粉磨站3#水泥库顶收尘器","FMD32-5","DA240","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[241,"三期粉磨站3#水泥库底收尘器","FMD32-6","DA241","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[242,"三期粉磨站1#水泥库顶收尘器","FMD32-5","DA242","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[243,"三期粉磨站1#水泥库底收尘器","FMD32-6","DA243","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[244,"三期粉磨站5#水泥库顶收尘器","FMD32-5","DA244","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[245,"三期粉磨站5#水泥库底收尘器","FMD32-6","DA245","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[246,"三期粉磨站4#水泥库顶收尘器","FMD32-5","DA246","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",11200,65,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[247,"三期粉磨站4#水泥库底收尘器","FMD32-6","DA247","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",13400,15,0.55,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[248,"一期成品斜槽头部新增收尘器","DMD96A","DA248","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5000-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[249,"2#SCR反应塔灰斗收尘器","DMD112A","DA249","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","10000-120000",15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[250,"3#SCR反应塔灰斗收尘器","DMD112A","DA250","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","10000-120000",15,0.4,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[251,"1#SCR反应塔灰斗收尘器","DMD112A","DA251","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","10000-120000",15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[252,"二期成品斜槽头部新增收尘器","DMD96A","DA252","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5000-7000",20,"0.3（方）","一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样至少3个样","《固定污染源废气 低浓度颗粒物的测定 重量法》（HJ836-2017）",1]
[253,"火炬燃烧废气排放口","-","DA253","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","-",15,0.6,"一般排放口",120,"重庆市《大气污染物综合排放标准》（DB 50/418-2016）","手工监测","半年/次","非连续采样 至少3个","固定污染源废气低浓度颗粒物的测定重量法HJ836-2022",4]
[{"$nulls":5},"二氧化硫","-",15,0.6,"一般排放口",550,"重庆市《大气污染物综合排放标准》（DB 50/418-2016）","手工监测","半年/次","非连续采样 至少3个","固定污染源废气 二氧化硫的测定 非分散红外吸收法HJ 629-2011",4]
[{"$nulls":5},"氮氧化物","-",15,0.6,"一般排放口",240,"重庆市《大气污染物综合排放标准》（DB 50/418-2016）","手工监测","半年/次","非连续采样 至少3个","固定污染源废气 氮氧化物的测定 非分散红外吸收法HJ 692-2014",4]
[254,"餐厨垃圾预处理系统排放口","ZYF-9C","DA254","烟气流速,烟气温度,烟气含湿量,烟道截面积","氨（氨气）",20000,25,0.8,"一般排放口","/","《恶臭污染物排放标准》   （GB 14554-93）","手工监测","半年/次","非连续采样 至少3个","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",4]
[{"$nulls":5},"硫化氢",20000,25,0.8,"一般排放口","/","《恶臭污染物排放标准》   （GB 14554-93）","手工监测","半年/次","非连续采样 至少3个","5.4.10.3亚甲基蓝分光光度法（B)",4]
[{"$nulls":5},"甲硫醇",20000,25,0.8,"一般排放口","/","《恶臭污染物排放标准》   （GB 14554-93）","手工监测","半年/次","非连续采样 至少3个","固定污染源废气 甲硫醇等8种含硫有机化合物的测定 气袋采样-预浓缩/气相色谱-质谱法（HJ 1078-2019）",4]
[{"$nulls":5},"颗粒物",20000,25,0.8,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","半年/次","非连续采样 至少3个","固定污染源废气低浓度颗粒物的测定重量法HJ836-2017",4]
[{"$nulls":5},"臭气浓度",20000,25,0.8,"一般排放口","/","《恶臭污染物排放标准》   （GB 14554-93）","手工监测","半年/次","非连续采样 至少3个","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",4]
[255,"3139铁质材料输送皮带收尘排放口","FMD32-4","DA255","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",8792,21,0.44,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",1]
[256,"2#带头部袋收尘排放口","JQM6×32","DA256","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",10473,15,0.5,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",1]
[257,"一级筛分机新增收尘器排放口","CD6D","DA257","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物",28000,15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",4]
[258,"A#水泥磨粉煤灰仓收尘器排放口","DMD96A","DA258","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5000-7000",31,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",1]
[259,"B#水泥磨粉煤灰仓收尘器排放口","DMD97A","DA259","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5000-7001",31,0.3,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",1]
[260,"1051新增收尘器排放口","DMD98A","DA260","烟气流速,烟气温度,烟气含湿量,烟道截面积","颗粒物","5000-7002",15,0.6,"一般排放口",20,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","两年/次","非连续采样 至少3个","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T 16157-1996",1]
[]
["重庆海创2024-2025年协同处置窑尾监测方案"]
[15,"1#线窑尾收尘器","CBMP240-2-2×4","DA015","烟气流速,烟气温度,烟气含湿量,烟道截面积","氯化氢（HCl)",760000,90,6,"主要排放口",10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","环境空气和废气 氯化氢的测定 离子色谱法HJ 549-2016代替HJ 549-2009",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","氟化氢（HF)",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物",{"$nulls":4},0.5,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","铊、镉、铅、砷及其化合物",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","总有机碳",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","二噁英类",{"$nulls":4},"0.1ngTEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","年/次","非连续采样至少3个样","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱-高分辨质谱法HJ/T 77.2-2008",2,"海创协同处置固危废"]
[15,"2#线窑尾收尘器","CBMP240-2-2×4","DA030","烟气流速,烟气温度,烟气含湿量,烟道截面积","氯化氢（HCl)",760000,90,6,"主要排放口",10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","环境空气和废气 氯化氢的测定 离子色谱法HJ 549-2016代替HJ 549-2009",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","氟化氢（HF)",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","大气固定污染源氟化物的测定离子选择电极法HJ/T 67-2001",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物",{"$nulls":4},0.5,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","铊、镉、铅、砷及其化合物",{"$nulls":4},1,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","空气和废气颗粒物中金属元素的测定 电感耦合等离子体发散光谱法HJ777-2015",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","总有机碳",{"$nulls":4},10,"水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","季度/次","非连续采样至少3个样","环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017",8,"海创协同处置固危废"]
[{"$nulls":4},"烟气流速,烟气温度,烟气含湿量,烟道截面积","二噁英类",{"$nulls":4},"0.1ngTEQ/m3","水泥窑协同处置固体废物污染控制标准（GB30485-2013）","手工监测","年/次","非连续采样至少3个样","环境空气和废气 二噁英类的测定 同位素稀释高分辨气相色谱-高分辨质谱法HJ/T 77.2-2008",2,"海创协同处置固危废"]

{"sheet":"废气无组织","index":1,"n_rows":30,"n_cols":12,"rows_kept":30,"merged":[[0,0,0,11]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（无组织废气）"]
["序号","监测位置","监测内容","污染物名称","限值(mg/m3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[1,"主厂区东侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[2,"主厂区西侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[3,"主厂区南侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[4,"主厂区北侧","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[5,"粉磨站1#厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[6,"粉磨站2#厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[7,"矿山分厂西侧厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[8,"矿山分厂南侧厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[9,"矿山分厂北侧厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[10,"矿山分厂东北侧厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[11,"砂岩矿山1#厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[12,"砂岩矿山2#厂界","风速、风向","颗粒物",0.5,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","季度/次","非连续采样至少3个样","环境空气 总悬浮颗粒物的测定 重量法 GB/T 15432-1995",8]
[13,"主厂区东侧","风速、风向","氨",1,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","一年/次","非连续采样至少3个样","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",2]
[14,"主厂区西侧","风速、风向","氨",1,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","一年/次","非连续采样至少3个样","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",2]
[15,"主厂区南侧","风速、风向","氨",1,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","一年/次","非连续采样至少3个样","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",2]
[16,"主厂区北侧","风速、风向","氨",1,"重庆市水泥工业大气污染物排放标准(DB 50 656-2016)","手工监测","一年/次","非连续采样至少3个样","空气和废气 氨的测定 纳氏试剂分光光度法 HJ 533-2009",2]
[17,"主厂区东侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","5.4.10.3亚甲基蓝分光光度法（B)",2]
[18,"主厂区西侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","5.4.10.3亚甲基蓝分光光度法（B)",2]
[19,"主厂区南侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","5.4.10.3亚甲基蓝分光光度法（B)",2]
[20,"主厂区北侧","风速、风向","硫化氢",0.06," 恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","5.4.10.3亚甲基蓝分光光度法（B)",2]
[21,"主厂区东侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",2]
[22,"主厂区西侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",2]
[23,"主厂区南侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",2]
[24,"主厂区北侧","风速、风向","臭气浓度",10,"恶臭污染物排放标准（GB14554-1993）","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB T 14675-1993",2]
[25,"主厂区东侧","风速、风向","非甲烷总烃",4,"大气污染物综合排放标准(DB 50 418-2016)","手工监测","一年/次","非连续采样至少3个样"," 环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017                                                        ",2]
[26,"主厂区西侧","风速、风向","非甲烷总烃",4,"大气污染物综合排放标准(DB 50 418-2016)","手工监测","一年/次","非连续采样至少3个样"," 环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017                                                        ",2]
[27,"主厂区南侧","风速、风向","非甲烷总烃",4,"大气污染物综合排放标准(DB 50 418-2016)","手工监测","一年/次","非连续采样至少3个样"," 环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017                                                        ",2]
[28,"主厂区北侧","风速、风向","非甲烷总烃",4,"大气污染物综合排放标准(DB 50 418-2016)","手工监测","一年/次","非连续采样至少3个样"," 环境空气 总烃 甲烷和非甲烷总烃的测定 直接进样-气相色谱法 HJ604-2017                                                        ",2]

{"sheet":"厂界噪声","index":2,"n_rows":18,"n_cols":9,"rows_kept":18,"merged":[[0,0,0,8],[2,3,7,3],[9,3,17,3]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（噪声）"]
["序号","监测位置","监测内容","限值(dB)","执行标准","监测方式","监测频次","两年监测次数","备注"]
[1,"主厂区东侧","风速、风向","昼间:65dB；           夜间:55dB。","工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",4]
[2,"主厂区西侧","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[3,"主厂区南侧","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[4,"主厂区北侧","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[5,"粉磨站1#厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[6,"粉磨站2#厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[7,"矿山分厂南侧厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[8,"矿山分厂西侧厂界","风速、风向","昼间：60dB；           夜间：50dB。","工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[9,"矿山分厂北侧厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[10,"矿山分厂东北侧厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[11,"砂岩矿山1#厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[12,"砂岩矿山2#厂界","风速、风向",null,"工业企业厂界环境噪声排放标准（GB12348-2008）","手工监测","季度/次",8]
[13,"石灰石长皮带平硐噪声敏感点","风速、风向",null,"声环境质量标准（GB3096-2008）","手工监测","季度/次",8]
[14,"石灰石长皮带古池坝噪声敏感点","风速、风向",null,"声环境质量标准（GB3096-2008）","手工监测","季度/次",8]
[15,"石灰石长皮带廖山噪声敏感点","风速、风向",null,"声环境质量标准（GB3096-2008）","手工监测","季度/次",8]
[16,"石灰石长皮带新湾噪声敏感点","风速、风向",null,"声环境质量标准（GB3096-2008）","手工监测","季度/次",8]

{"sheet":"废水","index":3,"n_rows":152,"n_cols":10,"rows_kept":152,"merged":[[0,0,0,9],[2,1,9,1],[2,2,9,2],[2,5,9,5],[10,1,17,1],[10,2,17,2],[10,5,17,5],[18,1,25,1],[18,2,25,2],[18,5,25,5],[26,1,33,1],[26,2,33,2],[26,5,33,5],[34,1,41,1],[34,2,41,2],[34,5,41,5],[42,1,51,1],[42,2,51,2],[42,5,51,5],[52,1,61,1],[52,2,61,2],[52,5,61,5],[62,1,71,1],[62,2,71,2],[62,5,71,5],[72,1,81,1],[72,2,81,2],[72,5,81,5],[82,1,91,1],[82,2,91,2],[82,5,91,5],[92,1,101,1],[92,2,101,2],[92,5,101,5],[102,1,111,1],[102,2,111,2],[102,5,111,5],[112,1,121,1],[112,2,121,2],[112,5,121,5],[122,1,151,1],[122,2,151,2],[122,5,151,5]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（废水）"]
["序号","排口编号","监测内容","污染因子","限值(mg/L)","执行标准","监测方式","监测频次","两年监测次数","备注"]
[1,"生活区污水处理器（DW001）","流量、水温","PH值","6--9","污水综合排放标准GB8978-1996","手工监测","季度/次",8]
[2,null,null,"悬浮物",400,null,"手工监测","季度/次",8]
[3,null,null,"化学需氧量",500,null,"手工监测","季度/次",8]
[4,null,null,"五日生化需氧量",300,null,"手工监测","季度/次",8]
[5,null,null,"石油类",20,null,"手工监测","季度/次",8]
[6,null,null,"氟化物",20,null,"手工监测","季度/次",8]
[7,null,null,"氨氮","/",null,"手工监测","季度/次",8]
[8,null,null,"总磷","/",null,"手工监测","季度/次",8]
[9,"矿山生活污水处理设施","流量、水温","PH值","6--9","污水回用不外排","手工监测","半年/次",4]
[10,null,null,"悬浮物",400,null,"手工监测","半年/次",4]
[11,null,null,"化学需氧量",500,null,"手工监测","半年/次",4]
[12,null,null,"五日生化需氧量",300,null,"手工监测","半年/次",4]
[13,null,null,"石油类",20,null,"手工监测","半年/次",4]
[14,null,null,"氟化物",20,null,"手工监测","半年/次",4]
[15,null,null,"氨氮","/",null,"手工监测","半年/次",4]
[16,null,null,"总磷","/",null,"手工监测","半年/次",4]
[17,"码头污水处理设施","流量、水温","PH值","6--9","污水综合排放标准GB8978-1996","手工监测","季度/次",8]
[18,null,null,"悬浮物",400,null,"手工监测","季度/次",8]
[19,null,null,"化学需氧量",500,null,"手工监测","季度/次",8]
[20,null,null,"五日生化需氧量",300,null,"手工监测","季度/次",8]
[21,null,null,"石油类",20,null,"手工监测","季度/次",8]
[22,null,null,"氟化物",20,null,"手工监测","季度/次",8]
[23,null,null,"氨氮","/",null,"手工监测","季度/次",8]
[24,null,null,"总磷","/",null,"手工监测","季度/次",8]
[25,"制造分厂污水处理器","流量、水温","PH值","6--9","污水回用不外排","手工监测","半年/次",4]
[26,null,null,"悬浮物",400,null,"手工监测","半年/次",4]
[27,null,null,"化学需氧量",500,null,"手工监测","半年/次",4]
[28,null,null,"五日生化需氧量",300,null,"手工监测","半年/次",4]
[29,null,null,"石油类",20,null,"手工监测","半年/次",4]
[30,null,null,"氟化物",20,null,"手工监测","半年/次",4]
[31,null,null,"氨氮","/",null,"手工监测","半年/次",4]
[32,null,null,"总磷","/",null,"手工监测","半年/次",4]
[33,"餐厨垃圾污水处理排放口","流量,水温","PH值","6--9","污水综合排放标准GB8978-1996","手工监测","1次/季",8]
[34,null,null,"悬浮物",400,null,"手工监测","1次/季",8]
[35,null,null,"化学需氧量",500,null,"手工监测","1次/季",8]
[36,null,null,"五日生化需氧量",300,null,"手工监测","1次/季",8]
[37,null,null,"动植物油",100,null,"手工监测","1次/季",8]
[38,null,null,"氟化物",20,null,"手工监测","1次/季",8]
[39,null,null,"氨氮","/",null,"手工监测","1次/季",8]
[40,null,null,"总磷","/",null,"手工监测","1次/季",8]
[41,"熟料生产1#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[42,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[43,null,null,"COD",20,null,"手工监测","一年/次",2]
[44,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[45,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[46,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[47,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[48,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[49,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[50,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[51,"熟料生产2#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[52,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[53,null,null,"COD",20,null,"手工监测","一年/次",2]
[54,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[55,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[56,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[57,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[58,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[59,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[60,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[61,"水泥粉磨站1#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[62,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[63,null,null,"COD",20,null,"手工监测","一年/次",2]
[64,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[65,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[66,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[67,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[68,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[69,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[70,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[71,"水泥粉磨站2#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[72,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[73,null,null,"COD",20,null,"手工监测","一年/次",2]
[74,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[75,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[76,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[77,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[78,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[79,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[80,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[81,"水泥粉磨站3#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[82,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[83,null,null,"COD",20,null,"手工监测","一年/次",2]
[84,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[85,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[86,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[87,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[88,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[89,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[90,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[91,"石灰石矿山1#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[92,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[93,null,null,"COD",20,null,"手工监测","一年/次",2]
[94,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[95,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[96,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[97,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[98,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[99,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[100,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[101,"石灰石矿山2#雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[102,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[103,null,null,"COD",20,null,"手工监测","一年/次",2]
[104,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[105,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[106,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[107,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[108,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[109,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[110,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[111,"砂岩矿山雨水排放口","流量,水温","PH值","6-9","《地表水环境质量标准》（GB3838-2002） 三类","手工监测","一年/次",2]
[112,null,null,"溶解氧",5,null,"手工监测","一年/次",2]
[113,null,null,"COD",20,null,"手工监测","一年/次",2]
[114,null,null,"BOD5",5,null,"手工监测","一年/次",2]
[115,null,null,"氨氮",1,null,"手工监测","一年/次",2]
[116,null,null,"石油类",0.05,null,"手工监测","一年/次",2]
[117,null,null,"Cd",0.05,null,"手工监测","一年/次",2]
[118,null,null,"Hg",0.001,null,"手工监测","一年/次",2]
[119,null,null,"Pb",0.05,null,"手工监测","一年/次",2]
[120,null,null,"粪大肠菌群",10000,null,"手工监测","一年/次",2]
[121,"餐厨厂区地下水","流量、水温","pH","6.5≤pH≤8.5","《地下水质量标准》（GB/T 14848-2017）标准中表1及表2-Ⅲ类规定的限值。","手工监测","一年/次",2]
[122,null,null,"钾","/",null,"手工监测","一年/次",2]
[123,null,null,"钠",200,null,"手工监测","一年/次",2]
[124,null,null,"钙","/",null,"手工监测","一年/次",2]
[125,null,null,"镁","/",null,"手工监测","一年/次",2]
[126,null,null,"碳酸盐","/",null,"手工监测","一年/次",2]
[127,null,null,"碳酸氢盐","/",null,"手工监测","一年/次",2]
[128,null,null,"硫酸盐",250,null,"手工监测","一年/次",2]
[129,null,null,"氯化物",250,null,"手工监测","一年/次",2]
[130,null,null,"氨氮",0.5,null,"手工监测","一年/次",2]
[131,null,null,"Cl-",null,null,"手工监测","一年/次",2]
[132,null,null,"硝酸盐（氮）",20,null,"手工监测","一年/次",2]
[133,null,null,"挥发酚",0.002,null,"手工监测","一年/次",2]
[134,null,null,"氰化物",0.05,null,"手工监测","一年/次",2]
[135,null,null,"砷",10,null,"手工监测","一年/次",2]
[136,null,null,"汞",1,null,"手工监测","一年/次",2]
[137,null,null,"铬（六价）",0.05,null,"手工监测","一年/次",2]
[138,null,null,"总硬度",450,null,"手工监测","一年/次",2]
[139,null,null,"铅",10,null,"手工监测","一年/次",2]
[140,null,null,"氟化物",1,null,"手工监测","一年/次",2]
[141,null,null,"镉",5,null,"手工监测","一年/次",2]
[142,null,null,"铁",0.3,null,"手工监测","一年/次",2]
[143,null,null,"锰",0.1,null,"手工监测","一年/次",2]
[144,null,null,"铜",1,null,"手工监测","一年/次",2]
[145,null,null,"锌",1,null,"手工监测","一年/次",2]
[146,null,null,"镍",0.02,null,"手工监测","一年/次",2]
[147,null,null,"溶解性总固体",1000,null,"手工监测","一年/次",2]
[148,null,null,"耗氧量",3,null,"手工监测","一年/次",2]
[149,null,null,"总大肠菌群",3,null,"手工监测","一年/次",2]
[150,null,null,"石油类","/",null,"手工监测","一年/次",2]

{"sheet":"周边环境质量","index":4,"n_rows":6,"n_cols":8,"rows_kept":6,"merged":[[0,0,0,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（周边环境质量）"]
["序号","监测位置","监测介质","监测方式","监测指标","手工监测频次","两年监测次数","备注"]
[1,"青岭村一组","土壤","手工监测","汞、铊、镉、铅、砷、铍、铬、锡、锑、铜、钴、锰、镍、钒","一年/次",2]
[{"$nulls":4},"二噁英类","一年/次",2]
[2,"垃圾坑旁","土壤","手工监测","汞、铊、镉、铅、砷、铍、铬、锡、锑、铜、钴、锰、镍、钒","一年/次",2]
[{"$nulls":4},"二噁英类","一年/次",2]

{"sheet":"比对监测","index":5,"n_rows":41,"n_cols":13,"rows_kept":41,"merged":[[0,0,0,12],[2,0,9,0],[2,1,9,1],[2,2,9,2],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,8,4,8],[2,9,3,9],[5,4,8,4],[5,5,8,5],[5,6,8,6],[5,8,8,8],[6,9,7,9],[10,0,17,0],[10,1,17,1],[10,2,17,2],[10,4,11,4],[10,5,11,5],[10,6,11,6],[10,8,12,8],[10,9,11,9],[13,4,16,4],[13,5,16,5],[13,6,16,6],[13,8,16,8],[14,9,15,9],[18,0,25,0],[18,1,25,1],[18,2,25,2],[18,4,19,4],[18,5,19,5],[18,6,19,6],[18,8,20,8],[18,9,19,9],[21,4,24,4],[21,5,24,5],[21,6,24,6],[21,8,24,8],[22,9,23,9],[26,0,30,0],[26,1,30,1],[26,2,30,2],[26,4,27,4],[26,5,27,5],[26,6,27,6],[26,8,28,8],[26,9,28,9],[31,0,35,0],[31,1,35,1],[31,2,35,2],[31,4,32,4],[31,5,32,5],[31,6,32,6],[31,8,33,8],[31,9,33,9],[36,0,40,0],[36,1,40,1],[36,2,40,2],[36,4,37,4],[36,5,37,5],[36,6,37,6],[36,8,38,8],[36,9,38,9]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（比对监测）"]
["序号","在线设备","排口代码","参数","型号","厂家","产品编号","量程范围","监测采样要求","监测依据及方法","比对频次","两年监测次数","备注"]
[1,"1#线窑尾在线监测","DA015","流速","MODEL2010","北京雪迪龙科技股份有限公司","/","0-40m/s","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","/","0-15-45mg/m3",null,"固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"二氧化硫","MODEL1080UV","北京雪迪龙科技股份有限公司","/","0-70-400","一个生产周期内比对9组数据对","固定污染源废气 二氧化硫的测定定电位电解法/HJ57-2017 非分散红外吸收法/HJ629-2011","季度/次",8]
[{"$nulls":3},"NO",{"$nulls":3},"0-100-700",null,"固定污染源废气 氮氧化物的测定定电位电解法/HJ693-2014 非分散红外吸收法/HJ692-2014","季度/次",8]
[{"$nulls":3},"NO2",{"$nulls":3},"0-100-700",null,null,"季度/次",8]
[{"$nulls":3},"氧含量",{"$nulls":3},"0-25%",null,"5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"湿度",2062,"北京雪迪龙科技股份有限公司","/","0-40%","一个生产周期内比对5组数据对",null,"季度/次",8]
[2,"2#线窑尾在线监测","DA030","流速","MODEL2010","北京雪迪龙科技股份有限公司","2010A-R9-0778","0-40m/s","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","900CPMA-R9-0390","0-15-45mg/m3",null,"固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"二氧化硫","MODEL1080UV","北京雪迪龙科技股份有限公司","1080U-R9-0637","0-70-400","一个生产周期内比对9组数据对","固定污染源废气 二氧化硫的测定定电位电解法/HJ57-2017 非分散红外吸收法/HJ629-2011","季度/次",8]
[{"$nulls":3},"NO",{"$nulls":3},"0-100-700",null,"固定污染源废气 氮氧化物的测定定电位电解法/HJ693-2014 非分散红外吸收法/HJ692-2014","季度/次",8]
[{"$nulls":3},"NO2",{"$nulls":3},"0-100-700",null,null,"季度/次",8]
[{"$nulls":3},"氧含量",{"$nulls":3},"0-25%",null,"5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"湿度",2062,"北京雪迪龙科技股份有限公司","EPFX44124-04C","0-40%","一个生产周期内比对5组数据对",null,"季度/次",8]
[3,"3#线窑尾在线监测","DA040","流速","MODEL2010","北京雪迪龙科技股份有限公司","2010A-R9-0776","0-40m/s","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","900CPMA-R9-0389","0-15-45mg/m3",null,"固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[{"$nulls":3},"二氧化硫","MODEL1080UV","北京雪迪龙科技股份有限公司","1080U-R9-0639","0-70-400","一个生产周期内比对9组数据对","固定污染源废气 二氧化硫的测定定电位电解法/HJ57-2017 非分散红外吸收法/HJ629-2011","季度/次",8]
[{"$nulls":3},"NO",{"$nulls":3},"0-100-700",null,"固定污染源废气 氮氧化物的测定定电位电解法/HJ693-2014 非分散红外吸收法/HJ692-2014","季度/次",8]
[{"$nulls":3},"NO2",{"$nulls":3},"0-100-700",null,null,"季度/次",8]
[{"$nulls":3},"氧含量",{"$nulls":3},"0-25%",null,"5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"湿度",2062,"北京雪迪龙科技股份有限公司","EPFX44142-04C","0-40%","一个生产周期内比对5组数据对",null,"季度/次",8]
[4,"1#窑头在线监测","DA017","流速","MODEL2010","北京雪迪龙科技股份有限公司","/","0-40m/s","一个生产周期内比对5组数据对",null,"季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"湿度","MODEL2062","北京雪迪龙科技股份有限公司","/","0-40%",null,null,"季度/次",8]
[{"$nulls":3},"氧含量","MODEL2062","北京雪迪龙科技股份有限公司","/","0-25%","一个生产周期内比对9组数据对","5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","/","0-15-45mg/m3","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[5,"2#窑头在线监测","DA032","流速","MODEL2010","北京雪迪龙科技股份有限公司","2010A-R9-0770","0-40m/s","一个生产周期内比对5组数据对",null,"季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"湿度","MODEL2062","北京雪迪龙科技股份有限公司","229995Q","0-40%",null,null,"季度/次",8]
[{"$nulls":3},"氧含量","MODEL2062","北京雪迪龙科技股份有限公司","229995Q","0-25%","一个生产周期内比对9组数据对","5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","900CPMA-R9-0356","0-15-45mg/m3","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]
[6,"3#窑头在线监测","DA042","流速","MODEL2010","北京雪迪龙科技股份有限公司","2010A-R9-0768","0-40m/s","一个生产周期内比对5组数据对",null,"季度/次",8]
[{"$nulls":3},"温度",{"$nulls":3},"0-300℃",null,null,"季度/次",8]
[{"$nulls":3},"湿度","MODEL2062","北京雪迪龙科技股份有限公司","230527Q","0-40%",null,null,"季度/次",8]
[{"$nulls":3},"氧含量","MODEL2062","北京雪迪龙科技股份有限公司","230527Q","0-25%","一个生产周期内比对9组数据对","5.2.6.3电化学法测定氧（B)《空气和废气监测分析方法》（第四版）国家环境保护总局（2003年）","季度/次",8]
[{"$nulls":3},"颗粒物","SCS-900CPM","北京雪迪龙科技股份有限公司","900CPMA-R9-0364","0-15-45mg/m3","一个生产周期内比对5组数据对","固定污染源废气 低浓度颗粒物的测定重量法/HJ 836-2017","季度/次",8]

{"sheet":"油烟监测","index":6,"n_rows":14,"n_cols":12,"rows_kept":14,"merged":[[0,0,0,11],[2,1,4,1],[5,1,7,1],[8,1,10,1],[11,1,13,1]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（油烟监测）"]
["序号","监测位置","监测内容","污染物名称","限值(mg/m3)","执行标准","监测方式","监测频次","监测采样要求","监测依据及方法","两年监测次数","备注"]
[1,"矿山分厂食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[2,null,"风速、风向","非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[3,null,"风速、风向","臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]
[4,"专家公寓食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[5,null,"风速、风向","非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[6,null,"风速、风向","臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]
[7,"员工大食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[8,null,"风速、风向","非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[9,null,"风速、风向","臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]
[10,"水泥分厂食堂","风速、风向","油烟",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源废气 总烃、甲烷和非甲烷总烃的测定 气相色谱法 HJ38",2]
[11,null,"风速、风向","非甲烷总烃",0.5,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","固定污染源排气中颗粒物测定与气态污染物采样方法GB/T16157",2]
[12,null,"风速、风向","臭气浓度",80,"餐饮业大气污染物排放标准","手工监测","一年/次","非连续采样至少3个样","空气质量 恶臭的测定 三点比较式臭袋法 GB/T14675",2]

{"sheet":"个人剂量监测","index":7,"n_rows":8,"n_cols":9,"rows_kept":8,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["重庆海螺2024-2025年环境自行监测方案（个人剂量监测）"]
["序号","检测项目","姓名","检测/评价依据","检测方法","监测频次","职业类型","两年监测次数","备注"]
[1,"外照射个人剂量监测","李强","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业探伤（3B)",8]
[2,"外照射个人剂量监测","王金平","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业探伤（3B)",8]
[3,"外照射个人剂量监测","李云华","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业辐照（3A）",8]
[4,"外照射个人剂量监测","谭术平","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业辐照（3A）",8]
[5,"外照射个人剂量监测","张召彪","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业辐照（3A）",8]
[6,"外照射个人剂量监测","哈令新","GBZ128-2019  GB18871-2002","热释光个人剂量监测","一季度/次","工业辐照（3A）",8]

{"sheet":"场所辐射环境监测","index":8,"n_rows":7,"n_cols":10,"rows_kept":7,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["重庆海螺2024年环境自行监测方案（场所环境辐射监测）"]
["序号","监测位置","监测位置描述","监测项目","监测方法","监测方式","监测频次","监测评价依据","两年监测次数","备注"]
[1,"矿山长皮带1#X射线检测系统","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","年/次","《工业探伤放射防护要求标准》GBZ117-2022 ",2]
[2,"矿山长皮带2#X射线检测系统","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","年/次","《工业探伤放射防护要求标准》GBZ117-2022 ",2]
[3,"矿山一期0#带跨带仪放射源线检测系统","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","年/次","GBZ125-2009《含密封源仪表的放射卫生防护要求》",2]
[4,"矿山二期0#带跨带仪放射源线检测系统","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","年/次","GBZ125-2009《含密封源仪表的放射卫生防护要求》",2]
[5,"煤质分析仪","按照国家标准要求布置检测点位","工作场所\n辐射剂量水平","仪器法","手工监测","年/次","GBZ125-2009《含密封源仪表的放射卫生防护要求》",2]